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Kennel Unit Design Checklist
Perforated page — tear out & copy

Checklist details
Unit number:  ________________________________________________
Date of check:  ________________________________________________
Checked by:  ________________________________________________

Sleeping area
Dimensions: length m × width m = total m²:  ________________________________________________
[ ]  Floor area at least 1.9m² (new builds)
[ ]  Sufficient space for dog to sit, stand, lie flat, wag tail, walk, turn around
[ ]  Constant access (pop hole to exercise run)
[ ]  Bedding provided (vet-bed, raised bed, or similar)
[ ]  Water bowl available
[ ]  Lighting (natural or artificial)
[ ]  Ventilation (window, vent, mechanical)
[ ]  Draught-free (no gaps, no wind penetration)
Temperature within 10–26°C (record: morning / afternoon):  ________________________________________________

Exercise run
Dimensions: length m × width m = total m²:  ________________________________________________
[ ]  Fencing 1.8m high, no gaps, no climbable features
[ ]  Waterproof roof over at least 50% of the run
[ ]  Surface cleanable (concrete / paving / artificial turf)
[ ]  Visible to staff from corridor
[ ]  Secure gate (self-closing, lockable)
[ ]  Dig-proof (mesh at base, or paving)

Numbering and information
[ ]  Unit is clearly numbered (visible from corridor)
[ ]  Information posted (dog name, owner contact, vet, diet)
[ ]  Information retrievable in under 60 seconds

Result and signatures
Result:  PASS  /  PASS with notes  /  FAIL
Notes:
____________________________________________________________
____________________________________________________________
____________________________________________________________
Inspector signature / date:  ________________________________________________
Operator signature / date:  ________________________________________________
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